


**Steps to do before running calculations:**

****

****

Enable the movement of the adjacent boundary layer mesh with the moving face zone for the wall\_ablation dynamic zone

****